ADA Standards

604.3 – Clearance and size around the toilet – Make sure there is enough room for the user and the device.

A picture containing mirror, table

Description automatically generated

604.5 Grab bars – Important to know where we can have a grab bar and what size it can be.

A screenshot of a cell phone

Description automatically generatedA close up of text on a black background

Description automatically generated

604.4 Seats.  The seat height of a water closet above the finish floor shall be 17 inches (430 mm) minimum and 19 inches (485 mm) maximum measured to the top of the seat.  Seats shall not be sprung to return to a lifted position. – This is crucial when designing a seat that lifts and lowers the user.

Considering our starting budget to be 500$, it might be worth applying for a standard grant to receive an additional 500$. The documentation and application process could hold us back from applying.